**Vagabond 47 “Hei Matau” Data Sheet**

NEW VAGABOND 47, 1978, HULL BLUE, VELMARE, 1 x 120 HP PERKINS, BOW THRUSTER, 3 CABIN/S, 2 WC(S), 1

SHOWER CABIN, GENERATOR, WATER MAKER, AIR CONDITIONING, GPS INTERFACED WITH RADAR, RADAR,

SPINNAKER POLE IN ALUMINIUM, BOWSPRIT IN STEEL, MANUAL MAINSAIL, SAILS 1990, FULL RIGGING 2022,

BIMINI-TOP

**TECNHICAL DETAILS**

Year: **1978**

Category: **CRUISING**

Builder: **VELMARE**

Designer: **STEFINI**

Nr Guest cabin: **3**

Nr Guest wc: **2**

Engine: **1 x 120 PERKINS**

Lenght: **14,35**

Beam: **4,20**

Draft (mt): **1,95**

Hull color: **Blue**

Hull material: **FIBERGLASS**

Materiale coperta: **FIBERGLASS**

Colore Coperta: **White**

Price: **€ 79.000**

**INTERIORS**

Nr Guest cabin: **3**

Master Cabin: **Stern**

Nr Guest wc: **2**

Nr Guest Shower Box: **2 (ONE PER EACH WC)**

Bunk beds num.: **2**

Separate twin beds num.: **1**

Double bed no.: **1**

Interior finishes: **Composite and wood**

Upholstery: **Cotton**

Kitchen Accessories:

**Oven, Fridge, Gas hob,**

**Freezer, 2° fridge**

Amenities Equipments: **External speakers**

**ENGINES**

Engine number: **1**

Engine brand: **PERKINS**

Engine Power (HP): **120**

Fuel: **diesel**

Fuel Tank: **800**

Engine Hours: **3,800**

Engine maintenance - Year: **2022**

Fuel consumption Lt/h per engine: **7 (6,5 Knts)**

Batteries - Num.: **6**

Year of batteries: **2019=4 X SERVICES, 2020=1 X ENGINE, 2021= 1 X GENERATOR**

Transmission: **V-DRIVE**

Engine Propeller: **Fixed blades**

Bow thruster: **Ducted**

Fresh water tank (LT): **1.200**

Waste water tank?: **Yes FOR REAR WC**

**SYSTEMS AND INSTRUMENTS**

Systems:

**12V System, Boiler 220V, Engine Boiler, CQR Anchor, Second Anchor, Generator 4.5 Kw Mase, Air Conditioning, Bow anchor windlass, Battery Charger, Water maker (desalinator 40 Lt./hr), Air-Conditioner**

Equipment: **VHF (2), Radar, Compass**

Generator power, kw: **4,5**

Watermaker lt/h: **30**

**Electronic Brand:** **Raymarine ST6000**

GPS number: **2**

GPS Type: **Color, internal interfaced with Radar**

GPS inches: **10, internal/external**

Autopilot Type: **on sector**

**DECK AND HULL**

Antifouling - Year: **2022**

Sea water inlet material: **Bronze**

Lifting keel material: **Cast Iron**

Sea-cocks year: **2017**

Steering: **External**

Wheelhouse material: **wood**

Coverings:

**Sun awning, Bimini-top, Covering winch, Console coverage**

Accessories:

**Roll-Bar (2021), Tender, Outboard motor, Fold-away table**

Validity of RINA: **01/06/2025**

Life-raft validity ( > 12 miles 8 people): **01/07/2024**

**SAILS**

Sails:

MAINSAIL DACRON 1990

JIB DACRON 1990

STORM JIB DACRON 1990

GENNAKER NYLON 1990

Masts no.: **1**

Mast material: **aluminium**

**RIGGING**

Spinnaker Pole: **Alluminium**

BOWSPRIT: **Steel**

Mainsail type: **furling mast**

Furling main sail type: **Manual**

Furling jib type: **Manual**

Furling staysail type: **Manual**

Winch type: **Manual**

Rigging Equipment:

**Fore staysail, Manual**

**backstay**

Rigging: **Spiral**

Rigging year: **2022**